RADIAL ARM SAW SAFETY RULES

1.) Eye protection must be worn while operating the Radial Arm Saw.

2.) Always keep your hands out of the RED ZONE when the saw is in

operation.

3.) The Radial Arm Saw may be operated with the left or right arm, but

NEVER CUT WITH YOUR ARMS CROSSED.

4.) All adjustments MUST be made BEFORE turning the saw on.

5.) NO TALKING allowed when operating the saw.

6.) Allow the saw to reach FULL SPEED before starting the cut.

7.) Control the speed the saw cuts at. DO NOT let the saw accelerate

through the wood. This is controlled by maintaining a firm grip and

a stiff arm.

8.) Return the saw behind the fence after each cut is made.

9.) After all cuts are made, shut off the saw, return it behind the fence,

lock the machine in place, then let go of the handle. DO NOT at any

time, let go of the saw unless it is locked in the return position.

10.) The saw blade must be stopped before leaving the saw.

11.) Hold the wood firmly against the fence and table.

12.) Support long stock to keep it from rocking when being cut.

13.) A clamp should be used on the fence to cut several pieces the same

length.

14.) Ask permission of the instructor before using the Radial Arm Saw.

RADIAL ARM SAW SAFETY TEST

NAME:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

BLOCK:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

DATE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1) \_\_\_\_\_\_\_ (T/F) Eye protection must be worn while operating the Mitre Saw

2) \_\_\_\_\_\_\_ (T/F) Always keep your hands in the RED ZONE when the

saw is in operation.

3) \_\_\_\_\_\_\_ (T/F) The Radial Arm Saw may be operated with the left or

right arm, but NEVER cut with your arms crossed.

4) \_\_\_\_\_\_\_ (T/F) Adjustments can be made while the machine is

running.

5) \_\_\_\_\_\_\_ (T/F) Having a conversation while operating the machine is

safe.

6) \_\_\_\_\_\_\_ (T/F) Allow the saw to reach FULL SPEED before starting

the cut.

7) \_\_\_\_\_\_\_ (T/F) Control the speed the saw cuts at. DO NOT let the saw

accelerate through the wood. This is controlled by

maintaining a firm grip and a stiff arm.

8) \_\_\_\_\_\_\_ (T/F) After all cuts are made, shut off the saw, return it

behind the fence, lock the machine in place, then let

go of the handle. DO NOT at any time, let go of the

saw unless it is locked in the return position.

9) \_\_\_\_\_\_\_ (T/F) The blade must be running before leaving the saw.

10) \_\_\_\_\_\_\_ (T/F) Do not hold the wood firmly against the fence and

table.

11) \_\_\_\_\_\_\_ (T/F) Support long stock to keep it from rocking when

being cut.

12) \_\_\_\_\_\_\_ (T/F) A clamp should be used on the fence to cut several

pieces the same length.

13) \_\_\_\_\_\_\_ (T/F) Ask permission of the instructor before using the

Radial Arm Saw.

I saw the demonstration on \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(dd/mm/yyyy)