EDGE SANDER SAFETY RULES

1) The belt must be in good condition. Do not use the belt if it is torn, clogged,

 or burned.

2) Make sure there is clearance between the belt and the table.

3) Wear eye protection and open the dust gate when using this machine.

4) Make sure that the piece you are sanding is large enough so that you can

 hold it safely.

5) NEVER try to free-hand your work. Make sure it is resting against the table.

6) Keep the stock moving back and forth on the tale so you use the whole belt,

 instead of burning only one spot.

7) Make sure that the sander has come to a complete stop before you walk

 away. Especially because the motor controls both sanders.

8) Check to make sure that body is to the RIGHT or LEFT of you when you are

 using the machine. This is to ensure that if you lose your stock it will not hit

 somebody.

9) Do not drive a piece of wood into the moving belt, but ease it in slowly. The

 abrasive is very aggressive and this will cause the piece of wood to take off.

10) Make sure you have your long hair tied back, and that all loose clothing is

 tucked in so it is not to catch while the machine is operating.