DISK SANDER SAFETY RULES

1) The sanding disk must be in good condition. Don’t use the sander if the disk

 is loose, torn, burned, or clogged.

2) Make sure that there is a clearance between the disk and the table.

3) Wear eye protection when using the Disk Sander. It is still a cutting tool.

4) Keep all loose clothing away from the disk as it can get caught between the

 disk and the table.

5) Tie back long hair, or wear a hat over it.

6) NEVER stand to the sides of the disk sander when it is running. If the abrasive disk should come off, it will be thrown towards the edges or towards the sides of the sander.

7) Keep the material flat on the table. NEVER free-hand.

8) Keep stock out of the RED ZONE when sanding. The material on this side

 WILL be kicked up towards you because of the rotation.

9) Make sure the material is large enough to be held safely.

10) Keep the stock moving back and forth across the downward side of the

 disk. Holding it on one spot will cause it to burn.

11) Make sure that the sander has stopped before walking away, especially

 because the motor controls both sanders. If you need to, you can use the

 cleaner to stop the sander.